Downstream MER test.

Test at room temperature.

Full channel plan.

Test 1 RF port.