**Test Procedure – Line to Battery Backup & Battery to Line Transition**

**Notes**

* Test with dual and single supply configurations. Observe if they perform similarly.
* Do not forget to test with all configuration from 7 nodes to 1 node, with 7 nodes being the worst-case network topology.
* If nodes are not available, use a module-level network instead.